org.lsst.ccs.application.args=--alias focal-plane-sim --description FocalPlane --initialConfiguration "defaultInitial"
# This needs to be a system property to keep the DAQ driver happy.
system.property.org.lsst.ccs.run.mode=simulation
org.lsst.ccs.application.extends=focal-plane
# Probably this should become the default, since it is the only option supported.
org.lsst.ccs.ld.library.path=Daq4
# We will simulate 2 rafts, R10 and R22
org.lsst.ccs.subsystem.focal.plane.rafts=[R10:[ccdType:itl],R22:[ccdType:itl]]