org.lsst.ccs.application.args=--description FocalPlane --initialConfiguration "\
   DAQ:common|<instrument>|<instrument>-<site>,\
   Devices:<instrument>,\
   General:common|<instrument>|<instrument>-<site>,\
   HardwareId:<instrument>,\
   Instrument:<instrument>|<instrument>-<site>,\
   Limits:<instrument>,\
   RaftsLimits:<instrument>,\
   RaftTempControl:<instrument>,\
   RaftTempControlStatus:<instrument>,\
   Rafts:<instrument>|<instrument>-<site>,\
   RaftsPower:<instrument>,\
   Sequencer:common|v25,\
   build:<instrument>,\
   Visualization:<site>,\
   timers:<instrument>" --alias focal-plane-sim
# This needs to be a system property to keep the DAQ driver happy.
system.property.org.lsst.ccs.run.mode=simulation
org.lsst.ccs.application.extends=focal-plane
# Probably this should become the default, since it is the only option supported.
org.lsst.ccs.ld.library.path=Daq4
# We will simulate 2 rafts, R10 and R22
#org.lsst.ccs.subsystem.focal.plane.rafts=[R10:[ccdType:itl],R22:[ccdType:itl]]
org.lsst.ccs.config.remote=true

org.lsst.ccs.subsystem.agent.property.cluster=comcam
org.lsst.ccs.subsystem.agent.property.instrument=comcam
org.lsst.ccs.subsystem.agent.property.site=tucson
